Signal Name | Total Product Terms | Product Terms | Location | Power Mode | Pin Number | PinType | Pin Use
--- | --- | --- | --- | --- | --- | --- | ---
OPTCMD_Readysig | 1 | 1_1 | MC1 | STD |  | (b) | (b)
NIDAQLogiccomp/wdone | 1 | 2_1 | MC2 | STD | 71 | I/O | I
NIDAQLogiccomp/command_out<9> | 1 | 3_1 | MC3 | STD |  | (b) | (b)
NIDAQLogiccomp/command_out<8> | 1 | 4_1 | MC4 | STD |  | (b) | (b)
NIDAQLogiccomp/command_out<7> | 1 | 5_1 | MC5 | STD |  | (b) | (b)
NIDAQLogiccomp/command_out<6> | 1 | 6_1 | MC6 | STD |  | (b) | (b)
NIDAQLogiccomp/command_out<5> | 1 | 7_1 | MC7 | STD |  | (b) | (b)
NIDAQLogiccomp/command_out<4> | 1 | 8_1 | MC8 | STD | 74 | I/O | I
NIDAQLogiccomp/command_out<3> | 1 | 9_1 | MC9 | STD |  | (b) | (b)
NIDAQLogiccomp/command_out<2> | 1 | 10_1 | MC10 | STD |  | (b) | (b)
NIDAQLogiccomp/command_out<1> | 1 | 11_1 | MC11 | STD | 75 | I/O | I
NIDAQLogiccomp/command_out<15> | 1 | 12_1 | MC12 | STD |  | (b) | (b)
NIDAQLogiccomp/command_out<14> | 1 | 13_1 | MC13 | STD |  | (b) | (b)
NIDAQLogiccomp/command_out<13> | 1 | 14_1 | MC14 | STD | 76 | I/O | I
NIDAQLogiccomp/command_out<12> | 1 | 15_1 | MC15 | STD | 77 | I/O | I
NIDAQLogiccomp/command_out<11> | 1 | 16_1 | MC16 | STD |  | (b) | (b)
NIDAQLogiccomp/command_out<10> | 1 | 17_1 | MC17 | STD | 78 | I/O | I
EventReadysig/EventReadysig_RSTF | 1 | 18_1 | MC18 | STD |  | (b) | (b)

Signals Used By Logic in Function Block

1. DIOA<0>
2. DIOA<1>
3. DIOA<2>
4. DIOA<3>
5. DIOA<4>
6. DIOA<5>
7. DIOA<6>
8. DIOA<7>
9. DIOB<1>
10. DIOB<2>
11. DIOB<3>
12. DIOB<4>
13. DIOB<5>
14. DIOB<6>
15. DIOB<7>
16. EventReadoutsig
17. MainLogiccomp/MAINSTATE_FFd2
18. NIDAQLogiccomp/NI_Interfacecomp/p2state_FFd1
19. rst