### Logic

Signal Name | Total Pterms | Total Inputs | Function Block | Macrocell | Power Mode | Slew Rate | Pin Number | Pin Type | Pin Use | Reg Init State
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
BUF_NIDAQLogiccomp/wen | 2 | 3 | FB14 | MC13 | STD |  |  | (b) | (b) |
CTRL | 1 | 2 | FB11 | MC10 | STD | FAST | 64 | I/O | O |
DIOC<0> | 5 | 7 | FB16 | MC12 | STD | FAST | 98 | I/O | O | RESET
DIOC<1> | 5 | 7 | FB16 | MC11 | STD | FAST | 97 | I/O | O | RESET
DIOC<2> | 5 | 7 | FB16 | MC10 | STD | FAST | 96 | I/O | O | RESET
DIOC<3> | 5 | 7 | FB16 | MC8 | STD | FAST | 95 | I/O | O | RESET
DIOC<4> | 5 | 7 | FB16 | MC6 | STD | FAST | 94 | I/O | O | RESET
DIOC<5> | 5 | 7 | FB16 | MC5 | STD | FAST | 93 | I/O | O | RESET
DIOC<6> | 5 | 7 | FB16 | MC3 | STD | FAST | 92 | I/O | O | RESET
DIOC<7> | 5 | 7 | FB16 | MC2 | STD | FAST | 91 | I/O | O | RESET
DIOD<0> | 5 | 7 | FB14 | MC15 | STD | FAST | 107 | I/O | O | RESET
DIOD<1> | 5 | 7 | FB14 | MC14 | STD | FAST | 106 | I/O | O | RESET
DIOD<2> | 5 | 7 | FB14 | MC11 | STD | FAST | 105 | I/O | O | RESET
DIOD<3> | 5 | 7 | FB14 | MC10 | STD | FAST | 104 | I/O | O | RESET
DIOD<4> | 5 | 7 | FB14 | MC8 | STD | FAST | 103 | I/O | O | RESET
DIOD<5> | 5 | 7 | FB14 | MC6 | STD | FAST | 102 | I/O | O | RESET
DIOD<6> | 5 | 7 | FB14 | MC5 | STD | FAST | 101 | I/O | O | RESET
DIOD<7> | 5 | 7 | FB14 | MC3 | STD | FAST | 100 | I/O | O | RESET
EventReadoutsig | 1 | 3 | FB8 | MC3 | STD |  | 131 | I/O | I | RESET
EventReadysig | 2 | 2 | FB9 | MC18 | STD |  |  | (b) | (b) | RESET
EventReadysig/EventReadysig_RSTF | 1 | 2 | FB13 | MC18 | STD |  |  | (b) | (b) |
FIFO_D<0> | 1 | 2 | FB8 | MC10 | STD | FAST | 134 | I/O | O |
FIFO_D<10> | 1 | 2 | FB4 | MC6 | STD | FAST | 4 | I/O | O |
FIFO_D<11> | 1 | 2 | FB4 | MC8 | STD | FAST | 5 | I/O/GTS1 | O |
FIFO_D<12> | 1 | 2 | FB4 | MC12 | STD | FAST | 6 | I/O/GTS2 | O |
FIFO_D<13> | 1 | 2 | FB4 | MC14 | STD | FAST | 7 | I/O | O |
FIFO_D<14> | 1 | 2 | FB2 | MC2 | STD | FAST | 9 | I/O | O |
FIFO_D<15> | 1 | 2 | FB2 | MC3 | STD | FAST | 10 | I/O | O |
FIFO_D<1> | 1 | 2 | FB6 | MC2 | STD | FAST | 135 | I/O | O |
FIFO_D<2> | 1 | 2 | FB6 | MC3 | STD | FAST | 136 | I/O | O |
FIFO_D<3> | 1 | 2 | FB6 | MC5 | STD | FAST | 137 | I/O | O |
FIFO_D<4> | 1 | 2 | FB6 | MC6 | STD | FAST | 138 | I/O | O |
FIFO_D<5> | 1 | 2 | FB6 | MC8 | STD | FAST | 139 | I/O | O |
FIFO_D<6> | 1 | 2 | FB6 | MC10 | STD | FAST | 140 | I/O | O |
FIFO_D<7> | 1 | 2 | FB6 | MC14 | STD | FAST | 142 | I/O | O |
FIFO_D<8> | 1 | 2 | FB4 | MC2 | STD | FAST | 2 | I/O/GTS3 | O |
FIFO_D<9> | 1 | 2 | FB4 | MC5 | STD | FAST | 3 | I/O/GTS4 | O |
MainLogiccomp/MAINSTATE_FFd1 | 2 | 12 | FB6 | MC12 | STD |  |  | (b) | (b) | RESET
MainLogiccomp/MAINSTATE_FFd2 | 2 | 11 | FB11 | MC13 | STD |  |  | (b) | (b) | RESET
MainLogiccomp/MAINSTATE_FFd3 | 4 | 12 | FB6 | MC18 | STD |  |  | (b) | (b) | RESET
NICMD_Argsig<0> | 2 | 4 | FB14 | MC12 | STD |  |  | (b) | (b) | RESET
NICMD_Argsig<1> | 2 | 4 | FB14 | MC9 | STD |  |  | (b) | (b) | RESET
NICMD_Argsig<2> | 2 | 4 | FB14 | MC7 | STD |  |  | (b) | (b) | RESET
NICMD_Argsig<3> | 2 | 4 | FB14 | MC4 | STD |  |  | (b) | (b) | RESET
NICMD_Argsig<4> | 2 | 4 | FB2 | MC17 | STD |  | 19 | I/O | I | RESET
NICMD_Argsig<5> | 2 | 4 | FB2 | MC16 | STD |  |  | (b) | (b) | RESET
NICMD_Argsig<6> | 2 | 4 | FB2 | MC15 | STD |  | 17 | I/O | I | RESET
NICMD_Argsig<7> | 2 | 4 | FB2 | MC14 | STD |  | 16 | I/O | I | RESET
NICMD_Readysig | 1 | 3 | FB14 | MC2 | STD |  |  | (b) | (b) | RESET
NICMDsig<0> | 2 | 4 | FB2 | MC13 | STD |  |  | (b) | (b) | RESET
NICMDsig<1> | 2 | 4 | FB2 | MC12 | STD |  | 15 | I/O | I | RESET
NICMDsig<2> | 2 | 4 | FB2 | MC11 | STD |  |  | (b) | (b) | RESET
NICMDsig<3> | 2 | 4 | FB2 | MC9 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NIDAQSTATE_FFd1 | 4 | 9 | FB14 | MC18 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NIDAQSTATE_FFd2 | 3 | 6 | FB14 | MC16 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NIDAQSTATE_FFd3 | 4 | 7 | FB14 | MC17 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<0> | 1 | 1 | FB10 | MC7 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<10> | 1 | 1 | FB7 | MC7 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<11> | 1 | 1 | FB9 | MC17 | STD |  | 59 | I/O | I | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<12> | 1 | 1 | FB9 | MC16 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<13> | 1 | 1 | FB9 | MC15 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<14> | 1 | 1 | FB9 | MC14 | STD |  | 58 | I/O | I | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<15> | 1 | 1 | FB9 | MC13 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<16> | 1 | 1 | FB10 | MC4 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<1> | 1 | 1 | FB9 | MC12 | STD |  | 57 | I/O | I | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<2> | 1 | 1 | FB9 | MC11 | STD |  | 56 | I/O | I | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<3> | 1 | 1 | FB9 | MC10 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<4> | 1 | 1 | FB9 | MC9 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<5> | 1 | 1 | FB9 | MC8 | STD |  | 54 | I/O | I | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<6> | 1 | 1 | FB9 | MC7 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<7> | 1 | 1 | FB9 | MC6 | STD |  | 53 | I/O | I | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<8> | 1 | 1 | FB9 | MC5 | STD |  | 52 | I/O | I | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack1_sync<9> | 1 | 1 | FB9 | MC4 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NI_Interfacecomp/ack2_sync | 1 | 1 | FB9 | MC3 | STD |  | 51 | I/O | I | RESET
NIDAQLogiccomp/NI_Interfacecomp/p2state_FFd1 | 1 | 3 | FB8 | MC2 | STD |  | 130 | I/O | I | RESET
NIDAQLogiccomp/NI_Interfacecomp/p2state_FFd2 | 2 | 3 | FB8 | MC12 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NI_Interfacecomp/p2state_FFd3 | 4 | 7 | FB8 | MC18 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NI_Interfacecomp/req2_cnt<0> | 1 | 2 | FB8 | MC1 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NI_Interfacecomp/req2_cnt<1> | 2 | 3 | FB8 | MC11 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NI_Interfacecomp/req2_cnt_ld | 1 | 1 | FB9 | MC2 | STD |  | 50 | I/O | I | SET
NIDAQLogiccomp/NumOfWordsSentCounter<0> | 2 | 3 | FB16 | MC18 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NumOfWordsSentCounter<1> | 2 | 4 | FB16 | MC17 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NumOfWordsSentCounter<2> | 2 | 5 | FB16 | MC16 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NumOfWordsSentCounter<3> | 2 | 6 | FB16 | MC15 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NumOfWordsSentCounter<4> | 2 | 7 | FB16 | MC14 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NumOfWordsSentCounter<5> | 2 | 8 | FB16 | MC13 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NumOfWordsSentCounter<6> | 2 | 9 | FB16 | MC9 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/NumOfWordsSentCounter<7> | 2 | 10 | FB8 | MC9 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeout | 1 | 17 | FB4 | MC3 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_0 | 1 | 2 | FB12 | MC2 | STD |  | 110 | I/O | I | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_10 | 2 | 3 | FB12 | MC17 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_11 | 2 | 4 | FB4 | MC18 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_12 | 2 | 5 | FB4 | MC17 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_13 | 2 | 6 | FB4 | MC16 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_14 | 2 | 7 | FB4 | MC15 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_15 | 2 | 8 | FB4 | MC13 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_1 | 2 | 3 | FB12 | MC18 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_2 | 2 | 4 | FB12 | MC16 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_3 | 2 | 5 | FB4 | MC11 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_4 | 2 | 7 | FB4 | MC10 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_5 | 2 | 3 | FB12 | MC15 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_6 | 2 | 4 | FB12 | MC14 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_7 | 2 | 5 | FB4 | MC9 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_8 | 2 | 6 | FB4 | MC7 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_0_9 | 2 | 8 | FB4 | MC4 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/Readtimeoutcounter_Madd__add0000__and0003/NIDAQLogiccomp/Readtimeoutcounter_Madd__add0000__and0003_D2 | 1 | 5 | FB12 | MC1 | STD |  |  | (b) | (b) |
NIDAQLogiccomp/Readtimeoutcounter_Madd__add0000__and0008/NIDAQLogiccomp/Readtimeoutcounter_Madd__add0000__and0008_D2 | 1 | 6 | FB4 | MC1 | STD |  |  | (b) | (b) |
NIDAQLogiccomp/Readtimeouten | 1 | 2 | FB14 | MC1 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/SendingPackageFlag | 3 | 11 | FB8 | MC17 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/StatusDatasig<0> | 2 | 2 | FB8 | MC7 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/StatusDatasig<10> | 2 | 2 | FB5 | MC14 | STD |  | 41 | I/O | I | RESET
NIDAQLogiccomp/StatusDatasig<11> | 2 | 2 | FB5 | MC13 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/StatusDatasig<12> | 2 | 2 | FB5 | MC12 | STD |  | 40 | I/O | I | RESET
NIDAQLogiccomp/StatusDatasig<13> | 2 | 2 | FB5 | MC11 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/StatusDatasig<14> | 2 | 2 | FB7 | MC18 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/StatusDatasig<15> | 2 | 2 | FB7 | MC17 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/StatusDatasig<1> | 2 | 2 | FB8 | MC6 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/StatusDatasig<2> | 2 | 2 | FB8 | MC4 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/StatusDatasig<3> | 2 | 2 | FB7 | MC16 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/StatusDatasig<4> | 2 | 2 | FB7 | MC15 | STD |  | 49 | I/O | I | RESET
NIDAQLogiccomp/StatusDatasig<5> | 2 | 2 | FB7 | MC14 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/StatusDatasig<6> | 2 | 2 | FB7 | MC13 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/StatusDatasig<7> | 2 | 2 | FB7 | MC12 | STD |  | 48 | I/O | I | RESET
NIDAQLogiccomp/StatusDatasig<8> | 2 | 2 | FB7 | MC11 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/StatusDatasig<9> | 2 | 2 | FB7 | MC10 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/cav | 1 | 2 | FB10 | MC3 | STD |  | 118 | I/O | (b) | RESET
NIDAQLogiccomp/command_out<0> | 1 | 1 | FB9 | MC1 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/command_out<10> | 1 | 1 | FB13 | MC17 | STD |  | 78 | I/O | I | RESET
NIDAQLogiccomp/command_out<11> | 1 | 1 | FB13 | MC16 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/command_out<12> | 1 | 1 | FB13 | MC15 | STD |  | 77 | I/O | I | RESET
NIDAQLogiccomp/command_out<13> | 1 | 1 | FB13 | MC14 | STD |  | 76 | I/O | I | RESET
NIDAQLogiccomp/command_out<14> | 1 | 1 | FB13 | MC13 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/command_out<15> | 1 | 1 | FB13 | MC12 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/command_out<1> | 1 | 1 | FB13 | MC11 | STD |  | 75 | I/O | I | RESET
NIDAQLogiccomp/command_out<2> | 1 | 1 | FB13 | MC10 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/command_out<3> | 1 | 1 | FB13 | MC9 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/command_out<4> | 1 | 1 | FB13 | MC8 | STD |  | 74 | I/O | I | RESET
NIDAQLogiccomp/command_out<5> | 1 | 1 | FB13 | MC7 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/command_out<6> | 1 | 1 | FB13 | MC6 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/command_out<7> | 1 | 1 | FB13 | MC5 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/command_out<8> | 1 | 1 | FB13 | MC4 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/command_out<9> | 1 | 1 | FB13 | MC3 | STD |  |  | (b) | (b) | RESET
NIDAQLogiccomp/wdone | 1 | 1 | FB13 | MC2 | STD |  | 71 | I/O | I | RESET
NIDAQLogiccomp/wen | 1 | 1 | FB16 | MC7 | STD |  |  | (b) | (b) | RESET
OEn | 0 | 0 | FB2 | MC8 | STD | FAST | 13 | I/O | O |
OPTCMD_Argsig<0> | 2 | 4 | FB5 | MC10 | STD |  | 39 | I/O | I | RESET
OPTCMD_Argsig<1> | 2 | 4 | FB12 | MC13 | STD |  |  | (b) | (b) | RESET
OPTCMD_Argsig<2> | 2 | 4 | FB12 | MC11 | STD |  |  | (b) | (b) | RESET
OPTCMD_Argsig<3> | 2 | 4 | FB12 | MC10 | STD |  | 115 | I/O | I | RESET
OPTCMD_Argsig<4> | 2 | 4 | FB12 | MC9 | STD |  |  | (b) | (b) | RESET
OPTCMD_Argsig<5> | 2 | 4 | FB12 | MC8 | STD |  | 113 | I/O | (b) | RESET
OPTCMD_Argsig<6> | 2 | 4 | FB12 | MC7 | STD |  |  | (b) | (b) | RESET
OPTCMD_Argsig<7> | 2 | 4 | FB12 | MC6 | STD |  |  | (b) | (b) | RESET
OPTCMD_Readysig | 1 | 1 | FB13 | MC1 | STD |  |  | (b) | (b) | RESET
OPTCMDsig<0> | 2 | 4 | FB6 | MC11 | STD |  |  | (b) | (b) | RESET
OPTCMDsig<1> | 2 | 4 | FB6 | MC9 | STD |  |  | (b) | (b) | RESET
OPTCMDsig<2> | 2 | 4 | FB6 | MC7 | STD |  |  | (b) | (b) | RESET
OPTCMDsig<3> | 2 | 4 | FB11 | MC9 | STD |  |  | (b) | (b) | RESET
OPTCMDsig<4> | 2 | 4 | FB11 | MC8 | STD |  |  | (b) | (b) | RESET
OPTCMDsig<5> | 2 | 4 | FB11 | MC7 | STD |  |  | (b) | (b) | RESET
OPTCMDsig<6> | 2 | 4 | FB11 | MC6 | STD |  |  | (b) | (b) | RESET
OPTCMDsig<7> | 2 | 4 | FB11 | MC5 | STD |  | 61 | I/O | I | RESET
OpticalLogiccomp/GenSimDatasig | 1 | 2 | FB7 | MC6 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/N0/OpticalLogiccomp/N0_D2 | 2 | 2 | FB7 | MC9 | STD |  |  | (b) | (b) |
OpticalLogiccomp/OPTICALLOGICSTATE_FFd1 | 2 | 11 | FB6 | MC4 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/OPTICALLOGICSTATE_FFd2 | 2 | 11 | FB6 | MC1 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/Busy | 1 | 2 | FB2 | MC4 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/EventReadyCmd | 1 | 2 | FB2 | MC1 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<0> | 1 | 1 | FB15 | MC18 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<10> | 1 | 1 | FB15 | MC17 | STD |  | 88 | I/O | I | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<11> | 1 | 1 | FB15 | MC16 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<12> | 1 | 1 | FB15 | MC15 | STD |  | 87 | I/O | I | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<13> | 1 | 1 | FB15 | MC14 | STD |  | 86 | I/O | I | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<14> | 1 | 1 | FB15 | MC13 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<15> | 1 | 1 | FB15 | MC12 | STD |  | 85 | I/O | I | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<1> | 1 | 1 | FB15 | MC11 | STD |  | 83 | I/O | I | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<2> | 1 | 1 | FB15 | MC10 | STD |  | 82 | I/O | I | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<3> | 1 | 1 | FB15 | MC9 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<4> | 1 | 1 | FB15 | MC8 | STD |  | 81 | I/O | I | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<5> | 1 | 1 | FB15 | MC7 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<6> | 1 | 1 | FB15 | MC6 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<7> | 1 | 1 | FB15 | MC5 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<8> | 1 | 1 | FB15 | MC4 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GLinkDatasig<9> | 1 | 1 | FB15 | MC3 | STD |  | 80 | I/O | I | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_0 | 1 | 2 | FB3 | MC3 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_10 | 2 | 4 | FB3 | MC17 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_11 | 2 | 5 | FB3 | MC16 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_12 | 2 | 6 | FB3 | MC15 | STD |  | 33 | I/O | I | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_13 | 2 | 7 | FB3 | MC13 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_14 | 2 | 8 | FB10 | MC18 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_15 | 2 | 9 | FB10 | MC16 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_1 | 2 | 3 | FB3 | MC18 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_2 | 2 | 4 | FB3 | MC12 | STD |  | 31 | I/O | I | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_3 | 2 | 5 | FB3 | MC11 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_4 | 2 | 6 | FB3 | MC10 | STD |  | 30 | I/O/GCK1 | GCK/I | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_5 | 2 | 7 | FB3 | MC9 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_6 | 2 | 8 | FB10 | MC15 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_7 | 2 | 9 | FB10 | MC13 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_8 | 2 | 11 | FB10 | MC9 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_0_9 | 2 | 3 | FB3 | MC8 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_Madd__add0000__and0007/OpticalLogiccomp/RxDataLogiccomp/GenDataCounter_Madd__add0000__and0007_D2 | 1 | 9 | FB3 | MC2 | STD |  | 28 | I/O | I |
OpticalLogiccomp/RxDataLogiccomp/GenDataDonesig | 1 | 16 | FB10 | MC1 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/RXDATALOGICSTATE_FFd1 | 2 | 4 | FB2 | MC7 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/RxDataLogiccomp/RXDATALOGICSTATE_FFd2 | 3 | 22 | FB2 | MC18 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/cnt<0> | 1 | 2 | FB7 | MC5 | STD |  | 46 | I/O | I | RESET
OpticalLogiccomp/TransmitCommandcomp/cnt<1> | 2 | 3 | FB3 | MC7 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/cnt<2> | 2 | 4 | FB3 | MC6 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/cnt<3> | 2 | 5 | FB3 | MC5 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/cnt<4> | 2 | 6 | FB3 | MC4 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/sending | 1 | 5 | FB3 | MC1 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<0> | 1 | 2 | FB7 | MC4 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<10> | 2 | 3 | FB1 | MC18 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<11> | 2 | 3 | FB1 | MC17 | STD |  | 27 | I/O | I | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<12> | 2 | 3 | FB11 | MC4 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<13> | 2 | 3 | FB11 | MC3 | STD |  | 60 | I/O | I | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<14> | 2 | 3 | FB1 | MC16 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<15> | 2 | 3 | FB1 | MC15 | STD |  | 26 | I/O | I | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<16> | 2 | 3 | FB1 | MC14 | STD |  | 25 | I/O | I | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<17> | 2 | 3 | FB1 | MC13 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<18> | 2 | 3 | FB11 | MC2 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<19> | 2 | 2 | FB11 | MC1 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<1> | 1 | 2 | FB7 | MC3 | STD |  | 45 | I/O | I | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<2> | 1 | 2 | FB7 | MC2 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<3> | 1 | 2 | FB7 | MC1 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<4> | 2 | 3 | FB1 | MC12 | STD |  | 24 | I/O | I | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<5> | 2 | 3 | FB1 | MC11 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<6> | 2 | 3 | FB1 | MC10 | STD |  | 23 | I/O | I | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<7> | 2 | 3 | FB1 | MC9 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<8> | 2 | 3 | FB1 | MC8 | STD |  | 22 | I/O | I | RESET
OpticalLogiccomp/TransmitCommandcomp/sr<9> | 2 | 3 | FB1 | MC7 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/command_insig<0> | 2 | 3 | FB1 | MC6 | STD |  | 21 | I/O | I | RESET
OpticalLogiccomp/command_insig<10> | 3 | 5 | FB6 | MC17 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/command_insig<11> | 3 | 5 | FB6 | MC16 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/command_insig<12> | 3 | 5 | FB6 | MC15 | STD |  | 143 | I/O/GSR | GSR/I | RESET
OpticalLogiccomp/command_insig<13> | 3 | 5 | FB6 | MC13 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/command_insig<14> | 3 | 5 | FB11 | MC18 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/command_insig<15> | 3 | 5 | FB11 | MC17 | STD |  | 70 | I/O | I | RESET
OpticalLogiccomp/command_insig<1> | 2 | 3 | FB12 | MC4 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/command_insig<2> | 2 | 3 | FB1 | MC5 | STD |  | 20 | I/O | I | RESET
OpticalLogiccomp/command_insig<3> | 2 | 3 | FB1 | MC4 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/command_insig<4> | 2 | 3 | FB1 | MC3 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/command_insig<5> | 2 | 3 | FB1 | MC2 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/command_insig<6> | 2 | 3 | FB1 | MC1 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/command_insig<7> | 2 | 3 | FB7 | MC8 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/command_insig<8> | 3 | 5 | FB11 | MC16 | STD |  |  | (b) | (b) | RESET
OpticalLogiccomp/command_insig<9> | 3 | 5 | FB11 | MC15 | STD |  |  | (b) | (b) | RESET
RCLK | 1 | 1 | FB2 | MC5 | STD | FAST | 11 | I/O | O |
RENn | 1 | 3 | FB2 | MC6 | STD | FAST | 12 | I/O | O | SET
REQ1 | 1 | 1 | FB12 | MC12 | STD | FAST | 116 | I/O | O | RESET
REQ2 | 1 | 1 | FB12 | MC3 | STD | FAST | 111 | I/O | O | RESET
RSTn | 0 | 0 | FB2 | MC10 | STD | FAST | 14 | I/O | O | RESET
SPARE<0> | 3 | 3 | FB10 | MC17 | STD | FAST | 129 | I/O | O | RESET
SPARE<10> | 2 | 4 | FB11 | MC11 | STD | FAST | 66 | I/O | O | RESET
SPARE<11> | 2 | 4 | FB5 | MC8 | STD | FAST | 38 | I/O/GCK3 | O | RESET
SPARE<12> | 2 | 4 | FB3 | MC14 | STD | FAST | 32 | I/O/GCK2 | O | RESET
SPARE<1> | 2 | 3 | FB10 | MC14 | STD | FAST | 128 | I/O | O | RESET
SPARE<2> | 2 | 3 | FB10 | MC12 | STD | FAST | 126 | I/O | O | RESET
SPARE<3> | 1 | 1 | FB10 | MC11 | STD | FAST | 125 | I/O | O | RESET
SPARE<4> | 1 | 3 | FB10 | MC10 | STD | FAST | 124 | I/O | O | RESET
SPARE<5> | 1 | 1 | FB10 | MC8 | STD | FAST | 121 | I/O | O | RESET
SPARE<6> | 1 | 1 | FB10 | MC6 | STD | FAST | 120 | I/O | O |
SPARE<7> | 1 | 1 | FB10 | MC5 | STD | FAST | 119 | I/O | O | RESET
SPARE<8> | 1 | 1 | FB11 | MC14 | STD | FAST | 69 | I/O | O |
SPARE<9> | 2 | 4 | FB11 | MC12 | STD | FAST | 68 | I/O | O | RESET
STOPTRIG1 | 0 | 0 | FB12 | MC5 | STD | FAST | 112 | I/O | O |
STOPTRIG2 | 0 | 0 | FB10 | MC2 | STD | FAST | 117 | I/O | O |
SendDataCmdsig | 1 | 1 | FB15 | MC2 | STD |  | 79 | I/O | I | RESET
StatusDatasig<0> | 3 | 5 | FB8 | MC16 | STD |  |  | (b) | (b) | RESET
StatusDatasig<10> | 2 | 4 | FB5 | MC9 | STD |  |  | (b) | (b) | RESET
StatusDatasig<11> | 2 | 4 | FB5 | MC7 | STD |  |  | (b) | (b) | RESET
StatusDatasig<12> | 2 | 4 | FB5 | MC6 | STD |  |  | (b) | (b) | RESET
StatusDatasig<13> | 2 | 4 | FB5 | MC5 | STD |  | 35 | I/O | I | RESET
StatusDatasig<14> | 2 | 4 | FB5 | MC4 | STD |  |  | (b) | (b) | RESET
StatusDatasig<15> | 2 | 4 | FB5 | MC3 | STD |  |  | (b) | (b) | RESET
StatusDatasig<1> | 3 | 5 | FB8 | MC15 | STD |  |  | (b) | (b) | RESET
StatusDatasig<2> | 3 | 5 | FB8 | MC14 | STD |  |  | (b) | (b) | RESET
StatusDatasig<3> | 3 | 5 | FB8 | MC13 | STD |  |  | (b) | (b) | RESET
StatusDatasig<4> | 3 | 5 | FB5 | MC18 | STD |  |  | (b) | (b) | RESET
StatusDatasig<5> | 3 | 5 | FB5 | MC17 | STD |  | 44 | I/O | I | RESET
StatusDatasig<6> | 3 | 5 | FB5 | MC16 | STD |  |  | (b) | (b) | RESET
StatusDatasig<7> | 3 | 5 | FB5 | MC15 | STD |  | 43 | I/O | I | RESET
StatusDatasig<8> | 2 | 4 | FB5 | MC2 | STD |  | 34 | I/O | I | RESET
StatusDatasig<9> | 2 | 4 | FB5 | MC1 | STD |  |  | (b) | (b) | RESET
WCLK | 1 | 1 | FB8 | MC8 | STD | FAST | 133 | I/O | O |
WENn | 1 | 2 | FB8 | MC5 | STD | FAST | 132 | I/O | O | SET