Pressure Test Plan
•	Calcs complete- submit E note for approval - may need to go to Kajiyama for review   
   Final note will have pressure test certs for all item below

•	Pressure vessel and Lid - change relief valve to 350 psi, ASME type  - use as is
•	Spool -  Fab (ASME cert. shop), assemble to octagon, blank off and test to 1.5x350 psi - tetest
•	Octagon, assemble to spool- test to 1.5x 350 psi - tetest
•	Feedthrus - SHV 20- make test chamber- test one to 4x350 psi or destruction if pass, test other two to 1.5x350 psi - tetest
•	Vac valve - use as is, with mfr cert.
•	Feedthrus - SHV 5 kV use as is, with mfr rating
•	CF-to-VCR fittings - assemble to each other and test 4x350 psi -tetest
•	PMT's - assemble test chamber  using 1.25" NPT class 1000 S.S. pipe and fitting, test to 350 psi using hand pump (88 has one) - ourselves (this is not part of pressure system)
•	Source tube- fab- assmeble with spool/octagon - test to 1.5x 350psi. If longer than spool, fab extension or buy nipple