### Summary

Design Name | top
Fitting Status | Successful
Software Version | I.31
Device Used | XC95288XL-6-TQ144
Date | 2-12-2007, 11:41AM

##### RESOURCES SUMMARY

Macrocells Used | Pterms Used | Registers Used | Pins Used | Function Block Inputs Used
--- | --- | --- | --- | ---
285/288 (99%) | 531/1440 (37%) | 255/288 (89%) | 115/117 (99%) | 474/864 (55%)

##### PIN RESOURCES

Signal Type | Required | Mapped
--- | --- | ---
Input | 57 | 57
Output | 56 | 56
Bidirectional | 0 | 0
GCK | 1 | 1
GTS | 0 | 0
GSR | 1 | 1
Pin Type | Used | Total
--- | --- | ---
I/O | 107 | 109
GCK/IO | 3 | 3
GTS/IO | 4 | 4
GSR/IO | 1 | 1

##### GLOBAL RESOURCES

Signal mapped onto global clock net (GCK1) | clk
Signal mapped onto global output enable net (GSR) | rst

##### POWER DATA

Macrocells in high performance mode (MCHP) | 285
Macrocells in low power mode (MCLP) | 0
Total macrocells used (MC) | 285